# lcxl3 custom-mode sniff
[DAW] note_on channel=15 note=11 velocity=127 time=0
[DAW] control_change channel=6 control=30 value=6 time=0
[DAW] note_on channel=15 note=11 velocity=0 time=0
[MIDI] SYSEX len=10 cmd=0x05 00 20 29 02 15 05 00 15 00 06
[MIDI] SYSEX len=10 cmd=0x05 00 20 29 02 15 05 00 15 03 06
